MODEL 66TKRW
KEY BENEFITS
BUSINESS SECTORS
• Provides comprehensive tracking and management-specific data particularly where the commission of the terrain above the Drilling head is not possible, such as when drilling under Water, roads, highways and other Surface obstacles when it is used with the 87B sonde.
FEATURES
• When combined use with a subsite horizontal sonde offers tracking device 66TKRW all locating important information, including position, Depth, roll angle, pitch, probe temperature and Battery status. In conjunction with the sonde 87B determines the tracking device, the Left / Right Deviation from the planned drilling length.
• The function "auto gain" holds the Sensitivity of the equipment is always at an optimal level in order to to achieve greater productivity.
• When equipped with the available as optional accessories Radio module can 66TKRW complete tracking information to the sub-site remote data-90D forward so that the operator of the drill drill head can see important information.
• The roll angle of the tool cutting edge is supported by a graphic digits with 12 segments shown.
• The slope is supported by pointing up / down Arrows as well as by numeric percentages shown.
RUGGED RELIABILITY
• Rugged housing for long life.
• Displays directions (roll angle, pitch, left / Right-deviation) within a 14-15 m wide Radius of the probe 87B through with minimal interference Metal structures in.
• Allows the commission to locate obstacles such as Highways, rail tracks, railways and buildings, when used in conjunction with the sonde 87B is used.
OPERATION
• LCD display provides a clear window for the current state of the hole.
• Probe depth is estimated by tapping a single button displayed.
• data with a user-selectable from two Channels are up to 610 m far transferred. Lightweight and with a good weight for practical use.
• When combined with the use of sonde 87B requires the operator of the locating device is not directly stand above the drill head to the probe data To receive left-right differences.
• Identifies critical drill information on practical Scheme and reliable way.
• Allows control of the drill head in difficult Locations.
• powered by standard alkaline cells.
• part of the subsite Total Tracking System
TECHNICAL
Dimensions
Length ................................................. .................................................. ............... 31 mm
Height ................................................. .................................................. ................ 71 mm
Width ................................................. .................................................. ................ 14 cm
Operating Weight ................................................. .......................................... 3.6 kilograms
Mode ................................................. .................................................. ................... Probe
Antenna configurations ................................ Up top, the bottom tip (automatic Selection)
Audio output ................................................. . Speakers; FM signal with four Volume settings
Frequencies ................................................. ...........................29 kHz, 33 kHz Internal Channel
Maximum Range ................................................ .................................................. ... 610 m
Batteries ................................................. .... Six C-mini-cells and two 9-volt Alkaline batteries
Typical battery life *
C-mini-cells ............................................. 16 hours without special accessories transmitter,
8 hours with transmitter 9-volt batteries, 60 hours Battery-saving device
The device switches off automatically 5 minutes if no button is pressed or no signal from the probe
Operating temperature range of the locating device ............................................... .. - 20 to 50 ° C
Storage temperature ................................................. ................................... - 30 to 60 ° C
Accuracy of depth estimation **
± 10 cm ............................................... .................................................. .. 10 cm to 3 m
± 5% ............................................... .................................................. ........... 3 to 6.1 m
± 10% ............................................... .................................................. .......... over 6.1 m
• Continuous operation at 21 ° C
The devices are calibrated to these tolerances under test field. Actual site conditions can lead to signal distortion or Noise sources included leading to depth estimates from the specified values differ.
PUSH BUTTON CONTROLS
Frequency. Overrides the automatic selection of the probe frequency Positioning device.
Automatic gain. Fits Gain on signal strength of At 45-55%.
Depth / calibration. For probe depth is estimated at Einzeltast - terminal device and the implementation of a ghost signal test. If in Conjunction with the left / right initialization / calibration key used for depth calibration.
Left / Right-initialization / calibration. Is to initialize the left / right sonde function used. If in Conjunction with the Shadows / Calibration button to calibrate and the probe depth measurement used. Left / Right-initialization / Calibration button: Is used when used with the sonde 87B also for switching between degrees and percent of the Volume key.
Volume / units. If the volume of the locating device Sound signal one and switches the depth measurement units between Inches, feet and inches and the inches or metric units Meters around.
On / Off. Turns the device on or off. In order to conserve Batteries will turn the tracking device after five minutes without Activity automatically.
LCD DISPLAY
LCD bar display. Displays probe signal strength and positioning device amplification at.
Alphanumeric display. Depth, units of depth measurement, Signal strength, sound pitch, left / right probe variance.
Symbol Display. Spacecraft roll angle, probe pitch, left / right Probe deviation, battery state of probe and beacon, Probe temperature, ghost signal indicator, Sonde - frequency, antenna mode, volume level indicator for long-distance information errors.